GDi - Green Drive ISO 15552

The series Green Drive ISO 15552 is particularly indicated for the replacement of pneumatic actuators. The motors are available in 6 different sizes with two different flange dimensions: from 45x45mm up to 70x70mm. The available windings are both for high voltage (230/480 VAC) and for low voltage (24/48 VDC).