Ethernet/IP Gateway

In order to control the integrated drive motor with Ethernet/IP Master PLC, it is possibile to use a standard Gateway solution.
The NLi motor must be updated with the Extended PDO Firmware. Please contact NiLAB for the right firmware.

HMS X-gateway – CANopen Master – EtherNet/IP Adapter configuration

Starting configuration file for 1 axis::integrated_drive_motors:pdo_fixed_cobids_hms.zip