Mechanical Installation

Slider distance for parallel drive mounting

Whne the application needs tandem parallel configuration of the integrated drive linear motor, the two or more actuator must mounted guarantee the safety distance L3 to avoid the interaction between magnetic sliders.

MOTOR MODEL	NO INTERACTION	MEDIUM INTERACTION	STRONG INTERACTION
NLi080	> 35 mm	> 15 mm to 35 mm	< 15 mm
NLi120	> 65 mm	> 45 mm to 65 mm	< 45 mm

NLi080Q Fixing points

NLi080X Fixing points

NLi120Q Fixing points

NLi120X Fixing points

NLi080Q/X slider fixing point

Slider has M4 threaded hole at each slider ends.

slider_8.jpg

NLi120QX slider fixing point

Slider has M4 threaded hole at each slider ends.

slider_12.jpg