Operating condition

the integrated drive linear motor are qualified to work with ambient temperature from 0 to +40 degrees Celsius.
The temperature of the motor winding is measured and monitor using I2T algoirthm

The standard IP protection level is IP65.