Connectors

rotolinear_photo.jpg

Rotolinear motor has 3 x M12 connectors (standard version) and 4 x M12 connectors (CanOPEN version).
L1 and L2 are the status led for linear and rotary motor.

Connector	Function	Type
C1	Power connector	M12, 5 poles male
C2	Signal connector for linear side	M12, 8 poles female
C3	Signal connector for rotary side	M12, 8 poles female
C4	CanOPEN connector	M12, 5 poles female

For pinout of the connectors on the relative cable, please see: https://www.nilab.at/dokuwiki/doku.php?id=integrated_drive_motors:connection_system|