Electrical connection

Cables

The electrical connection of linear motors is performed with using of free cable ends. For specific wiring schematic, please check the relevant documentation or contact the manufacturer.
The cable outlet is configurable. In the standard version, the cable outlet is placed parallel to x-axis, but other variants (y and z-axis) are also possible.

cable_exit.jpg

Power connection

L-series motors are normally provided with 1 m flexible shielded power cable without a connector (lead wires). Here is the meaning of the wire colors:

l_series_1.jpg

Please contact us to have the corresponding cable diameter in respect to the motor and winding code.

Power cable with connector

By request, L-series motors can be provided with 1 m flexible shielded power cable and a male Intercontec Speedtec series connector.

Lxxx-1215/2415/3615:

l_series_2.jpg

Lxxx-4815/6015:

l_series_3.jpg

How to assembly the power or signal connectors

Please refeer to the assembly istruction here: :ironcore_motors:montageanleitungen_gesamtkatalog.pdf