MBD 230/400 Servo Drive

mbd.jpg

MBD is a new range of low cost and high power Servo Drives. Five sizes are available, ranging from 3A to 42A continuous operation. The drive is offered with EtherCAT, CANopen or Analogue and includes a wide range of feedback options.

Controllable motors:

Brushless synchronous motors with torque, speed and position control

Brushless linear motors

Available motor feedback:

Encoder with Hall (standard)

SIN/COS 1Vpp

Absolute Hiperface

Catalogue Sheet

Hardware features

CAN Open slave (DS402 profile)

EtherCAT interface

Modbus RTU

A-B-Z type encoder emulation

Integrated clamp resistance with monitoring

5 opto-isolated inputs and 3 configurable outputs

2 inputs for disabling security STO A, STO B

2-line display

1 drive-ok relay

RS232 interface for configuration and data transfer

External power line for logical circuit (24 VDC)

Software features

absolute positioner on field bus interface (CAN open slave) or I/O with homing input

profile position mode, velocity mode and interpolation position mode

emergency braking with static position control

±10 V analog input

settable PID regulation

torque and speed control upon digital input

advanced function monitoring through RS232 interface with oscilloscope emulation