Installation

Slider distance for parallel drive mounting

When the application needs tandem parallel configuration of the integrated drive linear motor, the two or more actuators must be mounted guaranteeing the safety distance L3 to avoid the interaction between the magnetic sliders.

MOTOR MODEL	NO INTERACTION	MEDIUM INTERACTION	STRONG INTERACTION
NL040	> 20 mm	> 15 mm to 20 mm	< 10 mm
NL080	> 35 mm	> 15 mm to 35 mm	< 15 mm
NL120	> 65 mm	> 45 mm to 65 mm	< 45 mm

NL040Q Fixing points

nl40q_befest.jpg

NL040X Fixing points

nl40x_befest.jpg

NL080Q Fixing points

NL080X Fixing points

NL120Q Fixing points

NL120X Fixing points

NL040Q/X slider fixing point

Slider has M2 threaded hole at each slider ends.

nl040_rod_befest.jpg

NL080Q/X slider fixing point

Slider has M4 threaded hole at each slider ends.

slider_8.jpg

NL120QX slider fixing point

Slider has M4 threaded hole at each slider ends.

slider_12.jpg