Linear guide

lubrication_points.jpg

The linear guiding system is based on high performance Bosch Linear guides designed for high acceleration and high speed movements.
The system is composed by 4 linear guide blocks size 20 carbon steel (medium preload) with 4 independent lubrication nipples.

Lubrication use is Roller bearing grease Dynalub 510.

Linear guide performance

Parameter	Value	Unit
Maximum acceleration	500	m/sec
Maximum speed	5	m/sec
Dynamic load capacity per block C50	29.5	kN
Static load capacity per block C0	29.8	kN
Accuracy class	H
Preload class	C2
Permissible ambient temperature	-10 / +80	degrees
Typical lubrication frequency at high speed / high acceleration	1000	km