ULCO 44

Performance in a small size, ideal for small power application with limited space. Good load rating.

ulco44.jpg

Mechanical Drawing

ulco44_drw.jpg

Load rating

ulco44_forces.jpg

ulco44_rating.jpg

Technical data

Parameter	Symbol	Value	Unit
Max usable stroke	6500	mm
Total lenght	Ltot	C+Lc+210	mm
Carriage length	Lc	125	mm
Carriage usable length	Lu	110	mm
Extra-stroke (safety)	Ec	60	mm
Max speed	250	m/min
Max acceleration	100	m/sec2
Position repeatability	< 0.05	mm
Aluminium profile section	44 x 43	mm
Inertia momentum of aluminium profile	Ix	93110	mm4
Inertia momentum of aluminium profile	Iy	162710	mm4
Type of mechanic	linear guide with compact block
Belt type	Poliuretan HTD-5M-17
Pulley teeth number	24
Diameter	38,2	mm
Linear movement per rotation	120	mm
Operating temperature	-20 / +60	degrees