ULCO 132

Mechanical Drawing

Load rating

Technical data

Parameter	Symbol	Value	Unit
Max usable stroke	6500	mm
Total lenght	Ltot	C+Lc+260	mm
Carriage length	Lc	290	mm
Carriage usable length	Lu	270	mm
Extra-stroke (safety)	Ec	60	mm
Max speed	180	m/min
Max acceleration	100	m/sec2
Position repeatability	< 0.05	mm
Aluminium profile section	132 x 71 x 5	mm
Inertia momentum of aluminium profile	Ix	1413267	mm4
Inertia momentum of aluminium profile	Iy	2429437	mm4
Type of mechanic	linear guide with compact block
Belt type	Poliuretan HTD-5M-75
Pulley teeth number	36
Diameter	57,3	mm
Linear movement per rotation	180	mm
Operating temperature	-20 / +60	degrees