Connection system

Power cable - DE20001270-5M

The GDM linear unit is provided with two cables: power cable with PTC sensor connections.

l_series_1.jpg

Note: The thermal switch connections can be also in black color. In this case the cross-section of these wires are smaller than the motor phase wires.

Signal cable

lika_cable.jpg

Note: This signal cable can be provided with the connector type used from the servo drive.

Function	Cable wire colors
0 VDC	Black
+5VDC +/-5%	Red
SIN+	Yellow
SIN-	Blue
COS+	Green
COS-	Orange
Shielding	Shield